It is given that at the output of full converter Vmax must be less than 180 Vdc. We limited the duty cycle of buck converter to 80%. Then, Vrectifier,av can be calculate as below formula.

To obtain this average voltage the required input voltage voltage can be calculated as below formula.

Considering voltage drops on the diodes Vs was selected as 100 Vrms.